{"text_format":"1","workbook":"xlsx","n_sheets":1,"sheets":["XDisp Auto"],"not_rendered":{"charts":0,"images":0,"macros":1,"external_links":0,"defined_names":25,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900"}

{"sheet":"XDisp Auto","index":0,"n_rows":75,"n_cols":4,"rows_kept":75,"cut":false,"hidden":false,"merged":[]}
[]
[]
[null,null,"Example 1:","Open binary input data file, check data, analyse, save as new binary file."]
[]
[null,null,"Input File:","C:\\Program Files\\Oasys\\XDisp 20.2\\Samples\\Staged Construction\\Staged Construction - Simple.xdd"]
[null,null,"Output File:","C:\\Temp\\VBA_Example_1_Output.xdd"]
[]
[]
[]
[]
[]
[null,null,"Example 2:","Open JSON input data file, set volume loss of all tunnels, check data, analyse, save as new JSON data file."]
[]
[null,null,"Input File:","C:\\Program Files\\Oasys\\XDisp 20.2\\Samples\\Sample JSON.json"]
[null,null,"Output File:","C:\\Temp\\VBA_Example_2_Output.json"]
[null,null,"New Vol. Loss (%):",1]
[]
[]
[]
[]
[]
[null,null,"Example 3:","Open binary input data file, set all ground movement curves of all sides of all excavations, check data, analyse, save as new JSON data file."]
[]
[null,null,"Input File:","C:\\Program Files\\Oasys\\XDisp 20.2\\Samples\\Staged Construction\\Staged Construction - Simple.xdd"]
[null,null,"Output File:","C:\\Temp\\VBA_Example_3_Output.json"]
[null,null,"New GM Curve (V):",3]
[null,null,"New GM Curve (H):",3]
[]
[]
[]
[]
[]
[null,null,"Example 4:","Open JSON input data file, set E/G of all specific buildings, check data, analyse, save as new binary data file."]
[]
[null,null,"Input File:","C:\\Program Files\\Oasys\\XDisp 20.2\\Samples\\Sample JSON.json"]
[null,null,"Output File:","C:\\Temp\\VBA_Example_4_Output.xdd"]
[null,null,"New E/G:",2.1]
[]
[]
[]
[]
[null,null,"Example 5:","Open binary data file, set all specific utility acceptance criteria of all specific utilities, check data, analyse, save as new binary data file."]
[]
[null,null,"Input File:","C:\\Program Files\\Oasys\\XDisp 20.2\\Samples\\Staged Construction\\Staged Construction - Simple.xdd"]
[null,null,"Output File:","C:\\Temp\\VBA_Example_5_Output.json"]
[null,null,"New UAC Index:",10]
[]
[]
[]
[]
[null,null,"Example 6:","Open JSON data file, check data, analyse, set units for results' display, output to CSV all results' tables for the base model."]
[]
[null,null,"Input File:","C:\\Program Files\\Oasys\\XDisp 20.2\\Samples\\Sample JSON.json"]
[null,null,"Output File:","C:\\Temp\\VBA_Example_6_Output"]
[]
[]
[]
[]
[]
[null,null,"Example 7:","Open JSON data file, set units for results' display, output to CSV a Rail Track's cant results' table for one or all stages."]
[]
[null,null,"Input File:","C:\\Program Files\\Oasys\\XDisp 20.2\\Samples\\Sample JSON.json"]
[null,null,"Output File:","C:\\Temp\\VBA_Example_7_Output"]
[null,null,"Rail Track:",1]
[null,null,"Stage:",2]
[]
[]
[]
[]
[]
[null,null,"Example 8:","Open binary data file, check data, analyse, output all results' charts for one or all stages as image files."]
[]
[null,null,"Input File:","C:\\Program Files\\Oasys\\XDisp 20.2\\Samples\\Staged Construction\\Staged Construction - Simple.xdd"]
[null,null,"Output Folder:","C:\\Temp\\VBA_Example_8_Output"]
[null,null,"Stage:",0]